**LAB 3**

Read the ADC into channel 1 from a resister on your board

Left justify the information and remember to configure the input pin to be an analog input pin

Send the information to a port of your choosing and wire that port to the diodes